1.4Ton Excavator

|  |
| --- |
| Main Technical Specification |
| Dimension |
| Wheel Tread | mm | 1110 |
| Length of track | mm | 1420 |
| Ground clearance of upper platform | mm | 410 |
| Turning radius of tail | mm | 903 |
| Seat height | mm | 1620 |
| Width of track | mm | 180 |
| Height of track | mm | 320 |
| Transport length | mm | 3050 |
| Height | mm | 2350 |
| Driving speed | Km/h | 0-3km/h |
| Operating range |
| Maximum digging radius | mm | 3470 |
| Maximum digging depth | mm | 2150 |
| Maximum digging height | mm | 3040 |
| Maximum vertical digging depth | mm | 1520 |
| Min rotation radius | mm | 1340 |
| Height of bulldozing plate | mm | 345 |
| Depth of bulldozing plate | mm | 225 |
| Engine | **XINCHAI engine,three-cylinder engine,water-cool,Euro V.Emission** |
| Engine power | kw | 14 |
| Operation weight | kgs | 1400 |
| Bucket capacity | m³ | 0.03 |